Configurable Buffer.

Property: (default value)

Electric:

#include logicinputs
- Invert Inputs: (no)
   Invert input pins.
   
#include logicoutputs
#include gateoutputs
- Tristate: (no)
   If yes, creates an enable pin (active Low).
   When disabled, output is high impedance.

#include gatedelay
