eng	Pore color as a power of the Earlywood color (1.0 = same, < 1.0 = lighter, > 1.0 = darker).

eng	Power to compute pore color

eng	Depth

eng	Pore depth for bump effect.

eng	Bump depth variation (cm) for pores

eng	Earlywood only

eng	In both woods

eng	Latewood only

eng	Size

eng	Pore size.

eng	Radius (cm) of the impact circle of each pore

eng	Distribution

eng	Pores distribution.

eng	Pore type

eng	Earlywood only

eng	In both woods

eng	Latewood only

eng	Behavior

eng	Basic Thermal

eng	Mechanical

eng	Color Exponent

eng	Ray color as a power of the Earlywood color (1.0 = same, < 1.0 = lighter, > 1.0 = darker).

eng	Power to compute ray color

eng	Horizontal Size

eng	Ray horizontal size.

eng	Radius (cm) along the longer axis of ray ellipse

eng	Vertical Ratio

eng	Ray vertical stretching (1.0 = same, higher numbers = more stretching).

eng	Ratio between two radii of ray ellipse

eng	Density

eng	Number of rays along the circumference.

eng	Number of slices in xy plane

eng	Vertical Spacing

eng	Average vertical separation between rays.

eng	Length (cm) of z segment containing one ray

eng	Thickness (cm) of yearly growth ring

eng	Fibers Exponent

eng	Secondary highlights color as a power of the Earlywood color (1.0 = same). It can only be a lighter color.

eng	Power to compute secondary highlight color

eng	Use perlin noise for secondary highlight

eng	Variations Profile

eng	Variation profile describes the noise to apply to a value as a series of numeric pairs SS;WW, where SS is the Size and WW is the Weight. All values are in centimeters. For example 5.5;0.5 means that the noise size is 5.5cm and the value is shifted a maximum of 0.5cm. Multiple pairs can be specified to combine larger and smaller scale noises. For example, three different noises can be specified as 5.5;0.5;2.5;0.2;0.5;0.05 to combine large and smaller scale variations.

eng	Profile for secondary highlight perlin noise

eng	Vertical Scale

eng	Vertical highlights color variations stretching (1.0 = no stretching, smaller values = more stretching).

eng	Anisotropic pos-z scale for secondary highlight perlin

eng	Transforms

eng	Use additional groove roughness

eng	Use latewood bump

eng	Use manual latewood color

eng	Manual Latewood Color

eng	Enable to specify a custom Latewood color.

eng	Use pores feature

eng	Use rays feature

eng	HID Xenon

eng	yellow

eng	yellow-brown

eng	zinc

eng	ABS Plastic

eng	Acetal Resin, Black

eng	Acetal Resin, White

eng	Alloy Steel

eng	Aluminum-6061

eng	Aluminum-6061-AHC

eng	Brass, Soft Yellow

eng	Bronze, Soft Tin

eng	Carbon Steel

eng	Cast Bronze

eng	Cast Copper

eng	Cast Steel

eng	Copper

eng	Copper Alloy

eng	Ductile Iron

eng	Galvanized Steel

eng	GFRC (Glass Fiber Reinforced Concrete)

eng	Gold

eng	Gray Iron

eng	High Density Polyethylene

eng	High Impact Polystyrene

eng	LCP Plastic

eng	Lead

eng	Low Density Polyethylene

eng	Malleable Iron

eng	Nickel-Copper Alloy 400

eng	Non-Alloy Steel

eng	Nylon-6/6

eng	Nylon Composite (Nylon, molybdenum disulphide)

eng	PBT Plastic

eng	PC_ABS Plastic

eng	PET Plastic

eng	Phenolic

eng	PMMA Plastic

eng	Polycarbonate, Clear

eng	Polycarbonate, Smoke

eng	Polypropylene

eng	PPS Plastic

eng	PVC-Piping

eng	Rubber

eng	SAN Plastic

eng	Silicone

eng	Stainless Steel

eng	Stainless Steel, 440C

eng	Stainless Steel, Austenitic

eng	Steel, High Strength Low Alloy

eng	Steel, Mild

eng	UHMW, Black

eng	UHMW, White

eng	Welded Aluminum-6061

eng	Welded Brass, Soft Yellow

eng	Welded Stainless Steel, 440C

eng	Welded Steel Mild

eng	Wood (Birch)

eng	Wood (Cherry)

eng	Wood (Maple)

eng	Wood (Oak)

eng	Wood (Walnut)

eng	Wrought Copper

eng	Wrought Steel

eng	Threaded