Property: (default value)

- On Resistance: (500 Ω)
   Resistance when conducing.

- Off Resistance: (1e+08 Ω)
   Resistance when not conducing.

- Breakdwn Voltage (30 V)
    Voltage to start conducing.

- Holding Current: (0.01 A)
   Minimum current to keep conducing.


