Property: (default value)

Main:
- P Channel: (no)

- Depletion: (no)

Electric:
- RDSon: (1 Ω)
   DS Resistance in the lower part of the linear region when conducing:
    VGS > Vth and VDS < ( VGS – Vth )

- Threshold: (3 V)
   Gate-Source Voltage to start conducing.
