128x64 OLED monochrome graphic display.

Property: (default value)

- Color: (white)
   Pixel color.

- I2C Address: (62)
   Device address.

- I2C Frequency: (100 KHz)
   It is better to be similar to I2C Master frequency, but not critical in most cases.
