Inputs:
- Low to High Threshold: (2.5 V)
   Voltage to change from Low to High logic state.

- High to Low Threshold: (2.5 V)
   Voltage to change from High to Low logic state.

- Input Impedance: (1e+9 Ω)
   Impedance of digital input.
