Property: (default value)

Main:
- Tristate: (no)
   If yes, creates an enable pin (active Low).
   When disabled, output is high impedance.

#include gateinputs
Electric:
#include logicinputs
#include logicoutputs
#include logicedges
